**LED Blinking**

int LEDpin = 13;

int delayT = 1000;

void setup() {

// put your setup code here, to run once:

pinMode(LEDpin, OUTPUT);

}

void loop() {

// put your main code here, to run repeatedly:

digitalWrite(LEDpin, HIGH);

delay(delayT);

digitalWrite(LEDpin, LOW);

delay(delayT);

}