**DC Motor**

**[Note: This Program is same as LED blinking just replace LEDpin with DCMOTOR ]**

int DCMOTOR = 13;

int delayT = 1000;

void setup() {

// put your setup code here, to run once:

pinMode(DCMOTOR, OUTPUT);

}

void loop() {

// put your main code here, to run repeatedly:

digitalWrite(DCMOTOR, HIGH);

delay(delayT);

digitalWrite(LEDpin, LOW);

delay(delayT);

}